Phaseo Live Timing Bridge 0.1.0-beta

1. Extract the ZIP.
2. Run PhaseoLiveTimingBridge.exe.
3. Paste the bridge token shown in your Phaseo dashboard.
4. Enable UDP telemetry in F1 on port 20777 at 60 Hz.

Console players must run the bridge on a Windows PC on the same network and
set the in-game UDP address to that PC's local IPv4 address.
